**Owens Corning® Enclosure Solutions Wall System for Wood Stud Wall with High Compressive Mineral Wool Continuous Insulation (ci)**

**Specification Guide**

This specification guide presents in 3-part format all of the components of the Enclosure Solutions Wood Stud/High Compressive Mineral Wool ci Assembly. The components are presented in two MasterFormat Divisions: **Division 07 Thermal and Moisture Protection**.

System performance requirements are presented in **Division 01 Exterior Enclosure Performance Requirements** where all components are specified as a single system.

The major section headings provided are outlined below. Sections that require editing by the specifier are marked in **[highlighted bold with brackets].** Notes to the specifier are marked in [PINK with brackets.] Please note that edits to all Divisions are required to ensure complete performance of the system.

**Division 01 General Requirements:**Divisions 07 provided in this document outline complete 3-part MasterFormat sections for all components of a Wood Stud with high compressive mineral wool ci wall system.

Each of those sections cross reference back to the Division 01 Exterior Enclosure Performance Requirements to ensure that complete system performance requirements for building code compliance are concisely stated in the construction documents.

Include this section in your Project Manual to establish code compliance and complete system performance requirements.

**SECTION 01 83 16 EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS**

**Division 07 Insulation Components**:
This section includes Owens Corning® (OC) Thermafiber® RainBarrier® High Compressive Mineral Wool ci and, and OC EcoTouch® Fiberglas™ and/or OC) Thermafiber® UltraBatt™ Mineral Wool batt stud cavity insulations. This section outlines those products where they are commonly placed in the thermal insulation MasterFormat section:

**SECTION 07 21 13.19 MINERAL BOARD INSULATION and SECTION 07 21 16 BLANKET INSULATION**

Alternatively, the text for each product may be cut & pasted into their general MasterFormat Sections if desired:

**SECTION 07 21 00 THERMAL INSULATION**

**Division 07 Firestopping Components:**This section includes Owens Corning® (OC) Thermafiber® (mineral wool) Safing. This section outlines those products where they are commonly placed in the Firestopping MasterFormat section:

**SECTION 07 84 00 FIRESTOPPING**

Alternatively, for projects where both wall penetration firestopping and building perimeter firestopping are required, the text for each scope of work may be cut and pasted into more specific MasterFormat Section if desired:

**SECTION 07 84 13 PENETRATION FIRESTOPPING**

**PROJECT ARCHITECT RESPONSIBILITY:** This is a general specification guide, intended to be used by experienced construction professionals, in conjunction with good construction practice and professional judgment. This guide is to aid in the creation of a complete wall system specification that is to be fully reviewed and edited by the Architect of Record. Sections of this guide should be included, or edited, or omitted based on the requirements of a specific project. It is the responsibility of both the specifier and the purchaser to determine if a product or system is suitable for its intended use. Neither Owens Corning®, Thermafiber®, nor any of their subsidiary or affiliated companies, assume any responsibility for the content of this specification guide relative to actual projects, and specifically disclaim any and all liability for any errors or omissions in design, detail, structural capability, attachment details, shop drawings or other construction related details, whether based upon the information provided by the aforementioned companies or otherwise.

**SECTION 01 83 16 EXTERIOR ENCLOSURE PERFORMANCE REQUIRMENTS**

**PART 1 – GENERAL**

* 1. SUMMARY

Tested Wall System Description: Furnish and install specified products that have been tested to meet specified performance requirements for thermal, air, water, and fire resistance.

1. SECTION INCLUDES:
2. The complete wall system shall include the following:
3. **[Cladding & Cladding Attachment System]** over wood stud framed cavity wall by contractors.
4. Wood framing independently braced cavity to resist vertical and transverse structural loading.
5. Interior gypsum wallboard.
6. **[Faced, Unfaced] [Fiberglass, Mineral Wool, None]** Insulation batts in the framing cavity
7. Exterior sheathing with sealed joints.
8. Continuous air and water resistive barrier system applied to the exterior face of the sheathing wall installed in an airtight and flexible manner, allowing for the relative movement of systems due to thermal and moisture variations and capable of withstanding positive and negative combined wind, stack, and HVAC pressures on the envelope without damage or displacement.
9. Mineral Woolcontinuous insulation preliminarily secured to exterior sheathing with **[screws and air and water sealing washers, impaling pins attached with screws, impaling pins adhesively attached]** and permanently secured with **[cladding attachment system]**.
10. **[Safing to firestop the perimeter of door and window penetrations through wall.]**
11. **[Safing and sealant for sealing gaps between exterior wall and floor edge, perimeter fire containment system.]**
12. All joints, penetrations, and gaps of the air barrier wall system shall be made water and air tight.
	1. RELATED SECTIONS

Refer to the following Sections for additional requirements for each component in the assembly: [Delete section from the list below that are not required by the project.]

1. **Section 04 42 00 [Project Specific],** Exterior Stone Cladding
2. **Section 05 41 00 [Project Specific],** Structural Metal Stud Framing
3. **Section 05 50 00 [Project Specific],** Metal Fabrication (lintels, shelf angles, and masonry support)
4. **Section 06 11 00 [Project Specific],** Wood Framing
5. **Section 06 16 33 [Project Specific],** Wood Board Sheathing
6. **Section 07 05 43 [Project Specific],** Cladding Support Systems
7. **Section 07 10 00 [Project Specific],** Dampproofing and Waterproofing
8. **Section 07 21 00 [Project Specific],** Thermal Insulation
9. **Section 07 21 13.19 [Project Specific],** Mineral Board Insulation
10. **Section 07 21 16 [Project Specific],** Blanket Insulation
11. **Section 07 27 00 [Project Specific],** Air Barriers
12. **Section 07 42 00 [Project Specific],** Wall Panels
13. **Section 07 44 00 [Project Specific],** Faced Panels
14. **Section 07 46 00 [Project Specific],** Siding
15. **Section 07 50 00 [Project Specific],** Membrane Roofing
16. **Section 07 62 00 [Project Specific],** Sheet Metal Flashing and Trim
17. **Section 07 65 00 [Project Specific],** Flexible Flashings
18. **Section 07 84 00 [Project Specific],** Firestopping
19. **Section 07 92 00 [Project Specific],** Joint Sealants
20. **Section 09 29 00 [Project Specific],** Gypsum Board
21. **Section xx xx xx [Project Specific],** LEED Requirements

* 1. ADMINISTRATIVE REQUIREMENTS
1. COORDINATION

Coordinate installation of cladding, cladding attachment system, insulation, firestopping, and accessories with air barrier membrane, roofing, fenestration, and other moisture protection work.

1. PREINSTALLATION MEETINGS

Convene a meeting of involved sub-contractors a minimum of two weeks prior to commencing Work described in this Section.

1. Attendance is required by representatives of related trades including Owner’s Representative, Contractor, Architect, Installer, Air Barrier Membrane System Manufacturer, Roofing and Foundation Waterproofing Subcontractor, mechanical subcontractor, electrical contractor, and all subcontractors who have materials penetrating the air barrier membrane system or finishes covering the membrane system. Manufacturer’s Representative is available upon request with minimum two-week notice.
2. Contractor shall notify **[Architect, Engineer, Consultant]** at least 14 days prior to time for meeting.
3. Contractor shall record minutes of meeting and distribute to attending parties.
4. The agenda shall include at a minimum:
5. Materials proposed for use.
6. **[Verification of eligibility for any warranty].**
7. Sequence of construction.
8. Coordination with substrate preparation, condition, and pretreatment.
9. Compatibility of materials.
10. Air barrier requirements and installation.
11. Mechanical and electrical requirements and installation.
12. Minimum curing period.
13. Special details.
14. Mockups.
15. Air leakage and adhesion testing and inspection.
16. Air barrier protection and repair.
17. Work scheduling that covers air barrier coordination with installation of adjacent and covering materials.
18. Review and approval of all glazing applications.
19. Roofing installation.
	1. SUBMITTALS

Provide the following information in accordance with **Section 01 33 00 [Project Specific]** Submittal Procedures.

1. Product Data:

Submit product data of each component in tested wall assembly as required in **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. Shop Drawings (project-specific to air barrier assembly and Firestopping)

Submit shop drawings demonstrating tested wall assembly components as specified in **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. Samples:

Submit product minimum **[three]** samples of each component of the tested wall assembly system as required by this Section.

1. Certificates:

Submit documentation, signed by manufacturers, that products in tested wall assembly meet Quality Assurance Requirements as required in this Section.

1. Test AND EVALUATION Reports:

Submit manufacturer’s verification, test reports, or third-party engineering analysis that the proposed materials assembled as a tested wall system comply with the specified PERFORMANCE/ DESIGN CRITERIA of this Section.

1. MANUFACTURER’S INSTRUCTIONS

Provide installation instructions for all products in tested wall assembly as required in this Section.

1. SUSTAINABLE DESIGN SUBMITTALS:

Provide documentation of required Quality Assurance Sustainability Standards Certifications for all products in tested wall assembly as required in this Section.

1. SPECIAL PROCEDURE SUBMITTALS

None.

1. QUALIFICATION STATEMENTS

Provide documentation of required Quality Assurance Qualifications for Manufacturers and Installers for all products in tested wall assembly as required in this Section.

1. WARRANTY DOCUMENTATIOn

Submit sample warranties as required by this Section.

* 1. QUALITY ASSURANCE
1. QUALIFICATIONS

Manufacturers and Installers of specified products in the tested wall assembly shall meet Quality Assurance Qualifications requirements per **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. CERTIFICATIONS
2. Provide Manufacturer’s written certification that tested wall assembly components are compatible and provided as a single-source from the manufacturer.
3. Provide Manufacturer’s written certification that components are compatible with all adjacent materials that come into contact with the materials during construction and throughout the life of the building including insulation and attached membranes.
4. Provide Manufacturer’s written certification that products are for the intended purpose as described in this Section.
5. sustainability standards certifications

Provide documentation that specified products of the tested assembly meet Product Design/ Performance Criteria and Product Materials requirements of this Section and Quality Assurance Sustainability Standards Certifications of **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. mock-ups

Construct a wall system sample panel minimum 8 feet long x 8 feet high that includes wood stud framing, sheathing, air and water barrier, mineral wool continuous insulation, insulation fastening methods, through-

wall flashing, termination bars, drip edge, sealants, cladding attachment system, **[perimeter fire rated joint],** and cladding. The mock-up shall also include a window, storefront, or door frame, and sill opening transition assembly detailed with lintel, head, and sill flashings, and end dams to demonstrate surface preparation, crack and joint treatment, application of air barriers, and sealing of gaps, terminations, and penetrations of air-barrier assembly.

1. Coordinate construction of mockups to permit inspection by Owner's testing agency of air barrier before external insulation and cladding are installed.
2. Include transitions to roofing membrane, building corner condition, and foundation wall.
3. **[Architect, Engineer, Consultant]** approval of mockup is required. If it is determined that mockup does not comply with requirements, affected details must be reconstructed until mockups are approved.
4. Locate as directed and remove upon review and approval.
5. Approval of mockups does not constitute approval of deviations from the Contract Documents contained in mockups unless **[Architect, Engineer, Consultant]** specifically approves such deviations in writing. **[Indicate portion of wall represented by mockup on Drawings or draw mockup as separate element.]**

[Add note to indicate if ABAA's Quality Assurance Program is required.]

1. **[Subject to compliance with requirements, approved mockups may become part of the completed Work if undisturbed at time of Substantial Completion.]**
2. **[Preconstruction Testing Service: Owner will engage a qualified testing agency to perform preconstruction testing on field mockups.]**
3. DELIVERY, STORAGE, AND HANDLING

For specified products in the tested wall assembly, follow Delivery, Storage, and Handling requirements per **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. FIELD CONDITIONS

For specified products in the tested wall assembly, follow Field Conditions requirements per

**[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. WARRANTY
2. PRODUCT WARRANTY

Provide product warranties as required by **[Sections 04 20 00 Unit Masonry, 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. SYSTEM WARRANTY

Provide system warranty as required by **[Sections 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

1. INSTALLATION WARRANTY

Provide installation warranty as required by **[Sections 07 05 43 Cladding Support Systems, 07 21 00 Thermal Insulation, 07 27 00 Air Barriers, 07 42 00 Wall Panels, 07 44 00 Faced Panels, 07 46 00 Siding, and 07 84 13 Window/ Door/ Opening Penetration Firestopping].** [Insert all that apply from 1.2 RELATED SECTIONS.]

**PART 2 – PRODUCTS**

* 1. TESTED EXTERIOR WALL ASSEMBLY
1. MANUFACTURERS

BASIS-OF-DESIGN: Wood Stud Wall System.

1. Substitution Limitations

The “Basis of Design” tested wall assembly listed in this Section is tested as a system.  The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered:

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Provide and install wood stud framed exterior wall **[load-bearing, non-load bearing], [fire resistance rated, non-rated]** system, with air and water resistive barrier over the exterior sheathing, with mineral woolcontinuous insulation in the wall cavityand **[faced, unfaced]** **[fiberglass, mineral wool]** batt insulation in the stud cavity that effectively controls thermal, air, and water performance and provides continuous insulation and continuity of the building envelope.

1. PERFORMANCE/ DESIGN CRITERIA
2. FIRE CONTAINMENT AND RESISTANCE
	1. **[****NFPA 285 Limited Fire Propagation:
	Provide products that as a complete wall system pass NFPA 285, Standard Fire Test Method for Evaluation of Fire Propagation Characteristics of Exterior Non-Load-Bearing Wall Assemblies Containing Combustible Components.]** [If needed, refer to applicable building code for requirements.]
	2. **[ASTM E119 Fire Resistance:
	Provide products that as a system passes ASTM E119, Test Methods for Fire Tests of Building Construction and Materials.]** [If needed, refer to applicable building code for requirements.]
	3. **[ASTM E2307 Perimeter Fire Containment**

**Provide products that as a system passes ASTM E2307, Standard Test Method for Determining Fire Resistance of Perimeter Fire Barrier Systems Using Intermediate-Scale, Multistory Test Apparatus]** [If needed, refer to applicable building code for requirements.]

1. ASTM E2357 AIR LEAKAGE RESISTANCE

Provide a continuous air barrier as part of the tested wall system that has an air leakage not exceeding 0.004 cubic feet per square foot per minute under a pressure differential of 0.3 in. water (1.57 pounds per square foot) [0.20 liters per second per square meter at a pressure difference of 75 Pascals (0.20 L/(s·m²) @ 75 Pa)] when tested in accordance with ASTM E2357. Assembly shall accommodate movements of building materials by providing expansion and control joints as required.

1. ASTM E331 WATER PENETRATION

Provide a tested wall system tested in accordance with ICC-ES AC 212, Section 4.5, Acceptance Criteria for Water Resistive Coatings Used as Water Resistive Barriers over Exterior Sheathing, demonstrating that the system, tested in accordance with ASTM E331, shows no visible water penetration for 15 minutes at an air-pressure differential across the wall assembly of 2.86 psf (137 Pa), and 45 minutes at 6.27 psf (300 Pa).

1. THERMAL RESISTANCE

Provide a tested wall system that meets or exceeds code required R-value for exterior wall assemblies in the jurisdiction of the project. Submit manufacturer product data sheets and test reports prepared by a qualified testing agency to verify properties for insulation including R-value and other physical properties.

1. SOUND TRANSMISSION

Provide a tested wall system that meets or exceeds a Sound Transmission Class (STC) >55, and Outdoor Indoor Transmission Class (OITC) of >45 to >50 depending on wall design. Submit wall system engineering analysis or test reports for the wall assembly performed by qualified acoustical engineer or testing agency documenting STC and OITC classifications. [Include if STC and OITC are important to project performance. Refer to IBC 2015 Section 1207.]

1. INDOOR AIR QUALITY

Provide **[mineral wool, fiberglass]** insulation products that are formaldehyde free.

1. RECYCLED CONTENT

Provide insulation products **[fiberglass, mineral wool]** whose recycled content is verified via third party certification.

1. THIRD PARTY LISTING, CERTIFICATION, AND ENGINEERING JUDGEMENTS

Provide independent third-party verification listings or engineering judgements for the primary code requirements of **[NFPA 285 (fire propagation)]**, **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.

1. MATERIALS
2. **[Cladding & Cladding Attachment System]** over wood stud framed cavity wall by contractors.
3. Wood framing independently braced cavity to resist vertical and transverse structural loading.
4. Interior gypsum wallboard.
5. **[Faced, Unfaced] [Fiberglass, Mineral Wool]** Insulation batts in the framing cavity
6. Exterior wood sheathing with sealed joints.
7. Continuous air and water resistive barrier system applied to the exterior face of the sheathing wall installed in an airtight and flexible manner, allowing for the relative movement of systems due to thermal and moisture variations and capable of withstanding positive and negative combined wind, stack, and HVAC pressures on the envelope without damage or displacement.
8. Mineral Woolcontinuous insulation preliminarily secured to exterior sheathing with **[screws and air and water sealing washers, impaling pins attached with screws, impaling pins adhesively attached]** and permanently secured with **[cladding attachment system]**.
9. **[Safing to firestop the perimeter of door and window penetrations through wall.]**
10. **[Safing and sealant for sealing gaps between exterior wall and floor edge, perimeter fire containment system.]**

**PART 3 – EXECUTION- NOT USED**

**END OF SECTION 01 83 16**

**SECTION 07 21 13.19 MINERAL BOARD INSULATION**

**PART 1 – GENERAL**

* 1. SUMMARY

See Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, Section 01 83 16, **[including mandatory wall system compliance with NFPA 285 (fire spread)].** All proposed product substitutions must comply to be considered.

1. SECTION INCLUDES
2. Provide and install wood stud framed exterior wall **[load-bearing, non-load bearing], [fire resistance rated, non-rated]** system, with air and water resistive barrier over the exterior sheathing, with mineral woolcontinuous insulation in the wall cavityand **[faced, unfaced]** **[fiberglass, mineral wool]** batt insulation in the stud cavity that effectively controls thermal, air, and water performance and provides continuous insulation and continuity of the building envelope. Provide labor, materials, tools and equipment necessary to complete the Work of this Section including, but not limited to, the following:
3. Mineral wool continuous insulation for cavity wall application.
4. Fasteners and Hardware or other method as recommended by continuous insulation manufacturer.
5. The complete wall system shall include the following:
6. **[Cladding & Cladding Attachment System]** over wood stud framed cavity wall by contractors.
7. Wood framing independently braced cavity to resist vertical and transverse structural loading.
8. Interior gypsum wallboard.
9. **[Faced, Unfaced] [Fiberglass, Mineral Wool, None]** Insulation batts in the framing cavity
10. Exterior wood sheathing with sealed joints.
11. Continuous air and water resistive barrier system applied to the exterior face of the sheathing wall installed in an airtight and flexible manner, allowing for the relative movement of systems due to thermal and moisture variations and capable of withstanding positive and negative combined wind, stack, and HVAC pressures on the envelope without damage or displacement.
12. Mineral Woolcontinuous insulation preliminarily secured to exterior sheathing with **[screws and air and water sealing washers, impaling pins attached with screws, impaling pins adhesively attached]** and permanently secured with **[cladding attachment system]**.
13. **[Safing to firestop the perimeter of door and window penetrations through wall.]**
14. **[Safing and sealant for sealing gaps between exterior wall and floor edge, perimeter fire containment system.]**
15. All joints, penetrations, and gaps of the air barrier wall system shall be made water and air tight.
16. RELATED SECTIONS

The items listed are not included in this Section, but are specified in the Section listed: [Delete section from the list below that are not required by the project.]

1. **Section 04 42 00 [Project Specific],** Exterior Stone Cladding
2. **Section 05 41 00 [Project Specific],** Structural Metal Stud Framing
3. **Section 05 50 00 [Project Specific],** Metal Fabrication (lintels, shelf angles, and masonry support)
4. **Section 06 11 00 [Project Specific],** Wood Framing
5. **Section 06 16 33 [Project Specific],** Wood Board Sheathing
6. **Section 07 05 43 [Project Specific],** Cladding Support Systems
7. **Section 07 10 00 [Project Specific],** Dampproofing and Waterproofing
8. **Section 07 21 00 [Project Specific],** Thermal Insulation
9. **Section 07 21 16 [Project Specific],** Blanket Insulation
10. **Section 07 27 00 [Project Specific],** Air Barriers
11. **Section 07 42 00 [Project Specific],** Wall Panels
12. **Section 07 44 00 [Project Specific],** Faced Panels
13. **Section 07 46 00 [Project Specific],** Siding
14. **Section 07 50 00 [Project Specific],** Membrane Roofing
15. **Section 07 62 00 [Project Specific],** Sheet Metal Flashing and Trim
16. **Section 07 65 00 [Project Specific],** Flexible Flashings
17. **Section 07 84 00 [Project Specific],** Firestopping
18. **Section 07 92 00 [Project Specific],** Joint Sealants
19. **Section 09 29 00 [Project Specific],** Gypsum Board
20. **Section xx xx xx [Project Specific],** LEED Requirements

* 1. REFERENCES
1. REFERENCE STANDARDS

Materials shall meet the property requirements of one or more of the following specifications as applicable to the specific product or end use. [Delete references from the list below that are not required by the text of the edited Section.]

1. American Society for Testing of Materials (ASTM)
2. ASTM C165 Standard Test Method for Measuring Compressive Properties of Thermal Insulations
3. ASTM C356: Standard Test Method for Linear Shrinkage of Preformed High-Temperature Thermal Insulation Subjected to Soaking Heat.
4. ASTM C423 Standard Test Method for Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method
5. ASTM C518: Standard Test Method for Steady-State Thermal Transmission Properties by Means of Heat Flow Meter Apparatus.
6. ASTM C612: Standard Specification for Mineral Fiber Block and Board Thermal Insulation.
7. ASTM C665: Standard Specification for Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction and Manufactured Housing.
8. ASTM C795: Standard Specification for Thermal Insulation for Use in Contact with Austenitic Stainless Steel.
9. ASTM C954: Standard Specification for Steel Drill Screws for the Application of Gypsum Panel Products or Metal Plaster Bases to Steel Studs from 0.033 in (0.84 mm) to 0.112 in. (2.84 mm) in Thickness
10. ASTM C1104: Standard Test method for Determining the Water Vapor Sorption of Unfaced Mineral Fiber Insulation.
11. ASTM C1304 Standard Test Method for Assessing the Odor Emission of Thermal Insulation Materials
12. ASTM C1338 Standard Test Method for Determining Fungi Resistance of Insulation Materials and Facings
13. ASTM D1621: Standard Test Method for Compressive Properties of Rigid Cellular Plastics.
14. ASTM D4258: Standard Practice for Surface Cleaning Concrete for Coating
15. ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials
16. ASTM E96: Standard Test Methods for Water Vapor Transmission of Materials
17. ASTM E119: Standard Test Methods for Fire Tests of Building Constructions and Materials
18. ASTM E136: Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750°C.
19. National Fire Protection Association (NFPA)
20. NFPA 285: Standard Fire Method for Evaluation of Fire Propagation Characteristics of Exterior Non-Load-Bearing Wall Assemblies Containing Combustible Components.

* 1. ADMINISTRATIVE REQUIREMENTS
1. COORDINATION

Coordinate installation of insulation and accessories with cladding attachment system, air barrier membrane, and other moisture protection work.

1. PREINSTALLATION MEETINGS

Convene a meeting of involved sub-contractors a minimum of two weeks prior to commencing Work described in this Section.

1. Attendance is required by representatives of related trades including Owner’s Representative, Contractor, Architect, Installer, Air Barrier Membrane System Manufacturer, Roofing and Foundation Waterproofing Subcontractor, and all subcontractors who have materials penetrating the air barrier membrane system or finishes covering the membrane system. Manufacturer’s Representative is available upon request with minimum two week notice.
2. Contractor shall notify **[Architect, Engineer, Consultant]** at least 14 days prior to time for meeting.
3. Contractor shall record minutes of meeting and distribute to attending parties.
4. The agenda shall include at a minimum:
5. Materials proposed for use.
6. **[Verification of eligibility for any warranty].**
7. **[Engineering analysis provided by cladding attachment manufacturer for cladding and building conditions addressing fasteners and attachments].**
8. Sequence of construction.
9. Coordination with substrate preparation, condition, and pretreatment.
10. Compatibility of materials.
11. Air barrier requirements and installation.
12. Minimum curing period.
13. Special details.
14. Mockups.
15. Air leakage and adhesion testing and inspection.
16. Air barrier protection and repair.
17. Work scheduling that covers air barrier coordination with installation of adjacent and covering materials.
18. Review and approval of all glazing applications.
	1. SUBMITTALS

Provide the following information in accordance with **Section 01 33 00 [Project Specific]** Submittal Procedures.

1. Product Data: Manufacturers’ data on each type of product furnished including:
2. Preparation instructions and recommendations.
3. Technical data and tested physical and performance properties of products.
4. Storage, handling requirements, and recommendations.
5. Shop Drawings (project-specific to cladding and cladding attachment)
6. Show locations and extent of cladding attachment and cladding. Include details for substrate joints and cracks, counterflashing strips, penetrations, inside and outside corners, terminations, flashing transition assemblies, and tie-ins with adjoining construction.
7. Include details of interfaces with other materials that form part of building enclosure.
8. Samples: Submit product minimum **[three]** samples of the following:
9. Mineral Wool Insulation minimum **[three inches by three inches].**
10. Any fasteners, hardware, or other attachment methods recommended by manufacturer.
11. Certificates:

Submit documentation signed by Manufacturer that products meet Quality Assurance Certification requirements of this Section.

1. Test AND EVALUATION Reports:
2. **[NFPA 285: Provide documentation from qualified testing agency or fire engineer that the cladding, cladding attachment, insulation, and air barrier system as components of the designed wall assembly have been tested and passed NFPA 285 or approved by third-party engineering judgement.]**
3. ASTM C165: Provide documentation that the mineral wool continuous insulation meets minimum specified compressive strength requirements.
4. **[ASTM E119: Based on evaluation of comprehensive tests performed by a qualified testing agency, for assembly with specified fasteners, submit certified test report showing compliance with requirements specified for ASTM E119.]**
5. Engineering analysis: provide engineering analysis by cladding attachment manufacturer for cladding and building conditions using specified insulation, fasteners, cladding, and attachment accessories.
6. MANUFACTURER’S INSTRUCTIONS

Provide Manufacturer’s installation instructions for each product specified in this Section.

1. SUSTAINABLE DESIGN SUBMITTALS

Submit material health and recycled content of each product specified as required in Quality Assurance Sustainability Standards Certification of this Section.

**[LEED: Provide product prerequisite and/or credit summaries for each product specified as applicable including recycled content and Health Product Transparency information.]**

1. SPECIAL PROCEDURE SUBMITTALS

None.

1. QUALIFICATION STATEMENTS

Provide documentation of required Quality Assurance Qualifications for Manufacturers and Installers for all products in wall assembly as required in this Section.

1. WARRANTY DOCUMENTATIOn

Submit sample warranties as required by this Section.

* 1. QUALITY ASSURANCE
1. QUALIFICATIONS
2. MANUFACTURERS

Insulation systems shall be manufactured and marketed by a firm with a minimum of **[20]** years’ experience in the production and sales of insulation materials. Obtain continuous insulation material through one source from a single manufacturer. Manufacturers proposed for use, but not named in these specifications shall submit evidence of ability to meet all requirements specified and include a list of projects of similar design and complexity completed within the past **[five]** years.

1. INSTALLERS

The installation work of this section shall be performed by one entity, an experienced contractor that employs installers and supervisors who are trained and authorized by manufacturer, with a minimum **[two]** years’ record of successful installations on projects of similar scope.

1. CERTIFICATIONS
2. Provide Manufacturer’s written certification that cladding attachment system components are compatible.
3. Provide Manufacturer’s written certification that assembly components are compatible with all adjacent materials that come into contact during construction and throughout the life of the building.
4. Provide Manufacturer’s written certification that products are for the intended purpose as described in this Section.
5. SUSTAINABILITY STANDARDS CERTIFICATIONS
6. Minimum recycled content Certified by independent third-party testing.
7. Environmental Product Declaration.
8. MOCK-UPS

Construct a wall system sample panel minimum 8 feet long x 8 feet high that includes wood stud framing, sheathing, air and water barrier, mineral wool continuous insulation, insulation fastening methods, through-wall flashing, termination bars, drip edge, sealants, cladding attachment system, **[perimeter fire rated joint],** and cladding. The mock-up shall also include a window, storefront, or door frame, and sill opening transition assembly detailed with lintel, head, and sill flashings, and end dams to demonstrate surface preparation, crack and joint treatment, application of air barriers, and sealing of gaps, terminations, and penetrations of air-barrier assembly.

1. Coordinate construction of mockups to permit inspection by Owner's testing agency of air barrier before external insulation and cladding are installed.
2. Include transitions to roofing membrane, building corner condition, and foundation wall.
3. **[Architect, Engineer, Consultant]** approval of mockup is required. If it is determined that mockup does not comply with requirements, affected details must be reconstructed until mockups are approved.
4. Locate as directed and remove upon review and approval.
5. Approval of mockups does not constitute approval of deviations from the Contract Documents contained in mockups unless **[Architect, Engineer, Consultant]** specifically approves such deviations in writing.
6. **[Indicate portion of wall represented by mockup on Drawings or draw mockup as separate element.]**

[Add note to indicate if ABAA's Quality Assurance Program is required.]

1. **[Subject to compliance with requirements, approved mockups may become part of the completed Work if undisturbed at time of Substantial Completion.]**
2. **[Preconstruction Testing Service: Owner will engage a qualified testing agency to perform preconstruction testing on field mockups.]**
	1. DELIVERY, STORAGE, AND HANDLING
3. Deliver and store products in Manufacturer’s unopened packaging until ready for installation.
4. Store and protect products in accordance with Manufacturer’s instructions. Store in a dry area with adequate ventilation and protect from water and direct sunlight.
5. Remove and replace materials that are damaged.
	1. FIELD CONDITIONS
6. AMBIENT CONDITIONS
7. Apply products within the range of ambient and substrate temperatures recommended by manufacturer.
8. Protect substrates from environmental conditions that affect insulation performance.
	1. WARRANTY
9. MANUFACTURER WARRANTY
10. Product Warranty

Provide Manufacturer’s standard limited warranty against manufacturing defects.

**PART 2 – PRODUCTS**

* 1. MINERAL WOOL CONTINUOUS INSULATION
1. MANUFACTURERS

BASIS-OF-DESIGN: Owens Corning® ([www.owenscorning.com/insulation/commercial](https://www.owenscorning.com/insulation/commercial)) Thermafiber® RainBarrier ci High Compressive Max or equal product from one of the following:

1. **[Insert acceptable alternate supplier.]**
2. **[Insert acceptable alternate supplier.]**
3. Substitution Limitations

The “Basis of Design” products listed in this Section are tested and warranted as a system.  The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect,**

**Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Provide high compressive strength mineral wool continuous insulation, unfaced.

1. PERFORMANCE/ DESIGN CRITERIA
2. Type IA, IB, II, III, IVA, IVB per ASTM C612 certified by independent third-party testing agency.
3. Thermal Resistance (measured per ASTM C518 at mean temperature of 75F): R-4.2 per inch of thickness.
4. Compressive Strength (ASTM C165): Minimum 1200 pounds per square foot at 10% deflection
5. Water Sorption (ASTM C1104): Maximum 0.5 percent by volume.
6. Surface Burning Characteristics (ASTM E84): Flame spread maximum 0; smoke developed maximum 0, certified by independent third-party testing agency.
7. Sound Absorption (ASTM C423): Minimum 0.95 NRC at 2” thickness.
8. Corrosion of Steel, Aluminum, and Copper (ASTM C665): Pass.
9. Compatibility with Stainless Steel (ASTM C795): Pass.
10. Combustibility (ASTM E136): Non-Combustible per NFPA Standard 220.
11. Vapor Permeability (ASTM E96): Minimum 20 Perms.
12. Linear Shrinkage (ASTM C356): Less than 2% at 1200°F.
13. Fungi Resistance (ASTM C1338): Pass
14. Odor (ASTM C1304): Pass
15. Tested or Engineering Judgement per NFPA 285 as part of specified wall assembly.
16. MATERIALS
17. Recycle Content: Minimum **[70%, 75%]**, certified by independent third party such as ICC-ES.
18. Environmental Product Declaration (EPD) by independent third party such as UL Environment.
19. Provide R-4.2 per inch of thickness; **[1-1/4”, 1-1/2”, 2”, 2-1/2”, 3”, 3-1/2”, 4”]** thick; **[24”, 36”]** wide; **[48”, 72”]** long square edge.
	1. FASTENERS FOR MINERAL WOOL CONTINUOUS INSULATION
20. MANUFACTURERS
21. **[Insert acceptable alternate supplier.]**
22. **[Insert acceptable alternate supplier.]**
23. Substitution Limitations

The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Screw with Air & Water Sealing Washer: Provide preassembled screw and stress plate fasteners recommended by their manufacturer for securing mineral wool continuous insulation sheathing. Polymer or other corrosion-protected, coated steel screw fasteners for anchoring to sheathing and wood stud wall framing. Fastener length and size based on wall sheathing thickness and fastener manufacturer recommendation.

1. PERFORMANCE/ DESIGN CRITERIA
2. Tested per ASTM E331 as part of specified tested wall assembly.
3. Tested per ASTM E2357 as part of specified tested wall assembly.
4. MATERIALS
5. Screws for wood stud framing: Meet or exceed ASTM C954 and premium ceramic coating exceeds 1,000 hours of salt spray testing **[Zinc, Ceramic]** coated for corrosion protection.
6. Minimum 2 inch diameter air and water sealing washers: seal tested per ASTM E331 (water) and ASTM E2357 (air), **[pronged for ease of pre-positioning and easy on-the-wall screw assembly].**
7. Bugle head screws: Ranging from #6 - #10, coarse self-drilling for wood studs. Length of screw shall be one inch longer than the thickness of the insulation and wood sheathing combined for a minimum four threads of penetration through the wood studs.
	1. FASTENERS FOR MINERAL WOOL CONTINUOUS INSULATION
8. MANUFACTURERS
9. **[Insert acceptable alternate supplier.]**
10. **[Insert acceptable alternate supplier.]**
11. Substitution Limitations

The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Impaling Pin with Air & Water Sealing Washer: Provide preassembled screw and stress plate fasteners recommended by their manufacturer for securing mineral wool continuous insulation. Polymer or other corrosion-protected, coated steel screw fasteners for anchoring insulation to metal wall framing. Fastener length and size based on wall sheathing and insulation thickness and fastener manufacturer recommendation.

1. PERFORMANCE/ DESIGN CRITERIA
2. Tested per ASTM E331 as part of specified tested wall assembly.
3. Tested per ASTM E2357 as part of specified tested wall assembly.
4. MATERIALS
5. Screws for wood stud framing: Meet or exceed ASTM C954 and premium ceramic coating exceeds 1,000 hours of salt spray testing **[Zinc, Ceramic]** coated for corrosion protection.
6. 2 inch diameter air and water sealing washers: seal tested per ASTM E331 (water) and ASTM E2357 (air).
7. Bugle head screws: Ranging from #6 - #10, coarse self-drilling for wood studs. Length of screw shall be one inch longer than the thickness of sheathing for a minimum four threads of penetration through the wood studs.
8. Impaling needle minimum ½” greater than thickness of insulation.
9. Minimum 1” retaining washer or clip.
	1. FASTENERS FOR MINERAL WOOL CONTINUOUS INSULATION
10. MANUFACTURERS
11. **[Insert acceptable alternate supplier.]**
12. **[Insert acceptable alternate supplier.]**
13. Substitution Limitations

The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)],** ASTM E2357 (air leakage), and ASTM E331 (water penetration) requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Impaling Pin Adhesively Attached to Sheathing: Provide preassembled impaling pin and stress plate fasteners recommended by their manufacturer for securing mineral wool continuous insulation. Fastener length and size based on insulation thickness and fastener manufacturer recommendation.

1. PERFORMANCE/ DESIGN CRITERIA
2. Tested per ASTM E331 as part of specified tested wall assembly.
3. Tested per ASTM E2357 as part of specified tested wall assembly.
4. MATERIALS
5. 1 ½” inch or greater diameter air and water sealing washers: seal tested per ASTM E331 (water) and ASTM E2357 (air).
6. Impaling needle minimum ½” greater than thickness of insulation.
7. Minimum 1” retaining washer or clip.
8. Adhesive as recommended by manufacturer and approved by air and water barrier manufacturer.

**PART 3 – EXECUTION**

* 1. EXAMINATION
1. Verify that wall, opening framing, bridging and structural bracing, and other framing support members and anchorage have been installed per requirements of the Project.
2. Verify adjacent materials are dry and ready to receive insulation.
3. Do not begin installation until substrates have been properly prepared. If substrate preparation is the responsibility of another installer, notify owner’s agent and **[Architect, Engineer, Consultant]** of unsatisfactory preparation in writing before proceeding. Do not proceed with work until unsatisfactory conditions have been corrected.
4. Installation of products specified in this Section constitutes acceptance of existing conditions and assumption of responsibility for satisfactory performance.
	1. PREPARATION
5. Clean surfaces thoroughly prior to installation.
6. Prepare surfaces using methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	1. INSTALLATION
7. MINERAL WOOL CONTINUOUS INSULATION
8. Verify manufacturer recommended cure time for air and water barrier system before installing mineral wool continuous insulation board**.**
9. Install mineral wool continuous insulation boards over the exterior sheathing and air & water resistive barrier layer in accordance with manufacturers’ written recommendations.
10. Install mineral wool insulation board in maximum sizes to minimize joints.
11. Stagger joints.
12. Insulation board edges shall be butted together tightly and fit around openings and penetrations. Install square edges to fit square and tight.
13. Extend insulation in thickness indicated to envelop entire area to be insulated. Cut and fit tightly around obstructions and fill voids with insulation. Remove projections that interfere with placement.
14. Apply single layer of insulation boards to produce thickness indicated unless multiple layers are otherwise shown or required to make up total thickness.

[Owens Corning® does not require a particular method of securing Thermafiber® RainBarrier CI High Compressive Insulation, nor does Owens Corning® require joint sealing.]

1. Fasten mineral wool insulation to exterior face of wood stud wall framing and exterior sheathing using **[Screw and Air & water Sealing Washer, and/or Impaling Pin with Air & Water Sealing Washer, and/or Impaling Pin Attached with Adhesive]** per manufacturer’s written instructions. [Choose a, b, or c, or combination]
2. Screw with Air & Water Sealing Washer
3. Install through mineral wool insulation into sheathing and stud with self-drilling screws using a standard drill with a variable clutch adjustment and appropriate adapter or auto-feed fastening system.
4. Do not attach with impact driver.
5. Drive fasteners so the washer is tight and flush with insulation surface but do not countersink.
6. Impaling Pin with Air & Water Sealing Washer Attached with Screw
7. Install through sheathing and stud with self-drilling screws using a standard drill with a variable clutch adjustment and appropriate adapter or auto-feed fastening system.
8. Do not attach with impact driver.
9. Drive fasteners so the washer is tight and flush with exterior sheathing surface but do not countersink.
10. Install mineral wool insulation.
11. Slide metal washer over impaling pin to secure insulation in place.
12. Remove or bend protruding impaling pin as recommended by fastener manufacturer.
13. Impaling Pin Attached with Adhesive
14. Adhere impaling pin to sheathing per impaling pin manufacturer, air barrier manufacturer, and sheathing manufacturer recommendations.
15. Install mineral wool insulation.
16. Slide retaining clip over impaling pin to secure insulation in place.
17. Remove or bend protruding impaling pin as recommended by fastener manufacturer.
18. Fastener spacing shall be evenly distributed and the minimum necessary per job site conditions as required by Insulation Manufacturer to hold the continuous insulation in place until cladding attachment system can be installed to permanently secure the insulation board in accordance with **[Division 04 42 00, 07 05 43, 07 42 00, 07 44 00, 07 46 00]** requirements. **[Fastening requirements may be revised per job site conditions if insulation board is being installed at the same time as the cladding attachment system that will serve to secure insulation board to the substrate. Contractor must receive written confirmation from the [Architect, Engineer, Consultant] before altering fastener requirements.]**
19. **[Do not fasten more than one board edge with one fastener.]**
20. Install exterior veneer as soon as possible, best within 60 days.
	1. REPAIR
21. FILL ERRANT PUNCTURES, PENETRATIONS, AND HOLES
22. If fasteners are removed leaving penetration into the air barrier system beneath, the affected area must be detailed with air barrier sealant see **[Section 07 27 00 Air Barriers- Project Specific]** [Note: Fill of errant punctures, penetrations, and holes may be included in two separate specification sections and therefore

the responsibility of two separate trades. Identify the responsible trade according to project specific requirements.]

1. Completely fill the hole with sealant. Fill the hole in the continuous insulation board to full depth making sealant contact with the air and water barrier membrane below the insulation and fully flush with the outer face of the insulation.
	1. CLEANING
2. Prior to project closeout, remove all related rubbish, excess material, scaffolding, tools, and equipment from the site. Dispose of waste material in a manner approved by applicable jurisdictions.
	1. PROTECTION
3. Protect insulation from damage due to weather and physical abuse until protected by permanent construction.
4. Provide temporary coverings or enclosures where insulation is subject to abuse and cannot be concealed and protected by permanent construction immediately after installation.
5. Touch-up, repair, or replace damaged products before Substantial Completion.

**END OF SECTION 07 21 13.19**

**SECTION 07 21 16 BLANKET INSULATION**

**PART 1 – GENERAL**

* 1. SUMMARY

See Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, Section 01 83 16, **[including mandatory wall system compliance with NFPA 285 (fire spread)].** All proposed product substitutions must comply to be considered.

1. SECTION INCLUDES
2. Provide and install wood stud framed exterior wall **[load-bearing, non-load bearing], [fire resistance rated, non-rated]** system, with air and water resistive barrier over the exterior sheathing, with mineral woolcontinuous insulation in the wall cavityand **[faced, unfaced]** **[fiberglass, mineral wool]** batt insulation in the stud cavity that effectively controls thermal, air, and water performance and provides continuous insulation and continuity of the building envelope. Provide labor, materials, tools and equipment necessary to complete the Work of this Section including, but not limited to, the following:
3. **[Faced, Unfaced] [Fiberglas, Mineral wool]** batt insulation.
4. **[Fasteners and hardware or tape recommended by blanket insulation manufacturer.]**
5. The complete wall system shall include the following:
6. **[Cladding & Cladding Attachment System]** over wood stud framed cavity wall by contractors.
7. Wood framing independently braced cavity to resist vertical and transverse structural loading.
8. Interior gypsum wallboard.
9. **[Faced, Unfaced] [Fiberglass, Mineral Wool]** Insulation batts in the framing cavity
10. Exterior wood sheathing with sealed joints.
11. Continuous air and water resistive barrier system applied to the exterior face of the sheathing wall installed in an airtight and flexible manner, allowing for the relative movement of systems due to thermal and moisture variations and capable of withstanding positive and negative combined wind, stack, and HVAC pressures on the envelope without damage or displacement.
12. Mineral Woolcontinuous insulation preliminarily secured to exterior sheathing with **[screws and air and water sealing washers, impaling pins attached with screws, impaling pins adhesively attached]** and permanently secured with **[cladding attachment system]**.
13. **[Safing to firestop the perimeter of door and window penetrations through wall.]**
14. **[Safing and sealant for sealing gaps between exterior wall and floor edge, perimeter fire containment system.]**
15. All joints, penetrations, and gaps of the air barrier wall system shall be made water and air tight.
16. RELATED SECTIONS

The items listed are not included in this Section, but are specified in the Section listed: [Delete section from the list below that are not required by the project.]

1. **Section 04 42 00 [Project Specific],** Exterior Stone Cladding
2. **Section 05 41 00 [Project Specific],** Structural Metal Stud Framing
3. **Section 05 50 00 [Project Specific],** Metal Fabrication (lintels, shelf angles, and masonry support)
4. **Section 06 11 00 [Project Specific],** Wood Framing
5. **Section 06 16 33 [Project Specific],** Wood Board Sheathing
6. **Section 07 05 43 [Project Specific],** Cladding Support Systems
7. **Section 07 10 00 [Project Specific],** Dampproofing and Waterproofing
8. **Section 07 21 00 [Project Specific],** Thermal Insulation
9. **Section 07 21 13.19 [Project Specific],** Mineral Board Insulation
10. **Section 07 27 00 [Project Specific],** Air Barriers
11. **Section 07 42 00 [Project Specific],** Wall Panels
12. **Section 07 44 00 [Project Specific],** Faced Panels
13. **Section 07 46 00 [Project Specific],** Siding
14. **Section 07 50 00 [Project Specific],** Membrane Roofing
15. **Section 07 62 00 [Project Specific],** Sheet Metal Flashing and Trim
16. **Section 07 65 00 [Project Specific],** Flexible Flashings
17. **Section 07 84 00 [Project Specific],** Firestopping
18. **Section 07 92 00 [Project Specific],** Joint Sealants
19. **Section 09 29 00 [Project Specific],** Gypsum Board
20. **Section xx xx xx [Project Specific],** LEED Requirements

* 1. REFERENCES
1. REFERENCE STANDARDS

Materials shall meet the property requirements of one or more of the following specifications as applicable to the specific product or end use. [Delete references from the list below that are not required by the text of the edited Section.]

1. American Society for Testing of Materials (ASTM)
2. ASTM C423 Standard Test Method for Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method
3. ASTM C518: Standard Test Method for Steady-State Thermal Transmission Properties by Means of Heat Flow Meter Apparatus.
4. ASTM C612: Standard Specification for Mineral Fiber Block and Board Thermal Insulation.
5. ASTM C665: Standard Specification for Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction and Manufactured Housing.
6. ASTM C1104: Standard Test method for Determining the Water Vapor Sorption of Unfaced Mineral Fiber Insulation.
7. ASTM C1304: Standard Test Method for Assessing the Odor Emission of Thermal Insulation Materials
8. ASTM C1320: Standard Practice for Installation of Mineral Fiber Batt and Blanket Thermal Insulation for Light Frame Construction
9. ASTM C1338: Standard Test Method for Determining Fungi Resistance of Insulation Materials and Facings
10. ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials
11. ASTM E96: Standard Test Methods for Water Vapor Transmission of Materials
12. ASTM E119: Standard Test Methods for Fire Tests of Building Constructions and Materials
13. ASTM E136: Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750°C.
14. National Fire Protection Association (NFPA)
15. NFPA 101: Life Safety Code

* 1. ADMINISTRATIVE REQUIREMENTS
1. COORDINATION

Coordinate installation of insulation and accessories with air barrier membrane, roofing, fenestration, and other moisture protection work.

1. PREINSTALLATION MEETINGS

Convene a meeting of involved sub-contractors a minimum of two weeks prior to commencing Work described in this Section.

1. Attendance is required by representatives of related trades including Owner’s Representative, Contractor, Architect, Installer, Air Barrier Membrane System Manufacturer, Roofing and Foundation Waterproofing Subcontractor, mechanical subcontractor, electrical contractor, and all subcontractors who have materials penetrating the air barrier membrane system or finishes covering the membrane system. Manufacturer’s Representative is available upon request with minimum two-week notice.
2. Contractor shall notify **[Architect, Engineer, Consultant]** at least 14 days prior to time for meeting.
3. Contractor shall record minutes of meeting and distribute to attending parties.
4. The agenda shall include at a minimum:
5. Materials proposed for use.
6. **[Verification of eligibility for any warranty].**
7. Sequence of construction.
8. Coordination with substrate preparation, condition, and pretreatment.
9. Compatibility of materials.
10. Air barrier requirements and installation.
11. Mechanical and electrical requirements and installation.
12. Minimum curing period.
13. Special details.
14. Mockups.
15. Air leakage and adhesion testing and inspection.
16. Air barrier protection and repair.
17. Work scheduling that covers air barrier coordination with installation of adjacent and covering materials.
18. Review and approval of all glazing applications.
19. Roofing installation.
	1. SUBMITTALS

Provide the following information in accordance with **Section 01 33 00 [Project Specific]** Submittal Procedures.

1. Product Data: Manufacturers’ data on each type of product furnished including:
2. Preparation instructions and recommendations.
3. Technical data and tested physical and performance properties of products.
4. Storage, handling requirements, and recommendations.
5. Shop Drawings (project-specific to cladding and cladding attachment)
6. Show locations and extent of insulation installation. Include details for penetrations, inside and outside corners, terminations, transition assemblies, and tie-ins with adjoining construction.
7. Include details of interfaces with other materials that form part of building enclosure.
8. Samples: Submit product minimum **[three]** samples of the following:
9. **[Faced, Unfaced] [Fiberglas, Mineral]** wool batt insulation minimum **[three inches by three inches]**.
10. Any fasteners, recommended by manufacturer.
11. Certificates:

Submit documentation signed by Manufacturer that products meet Quality Assurance Certification requirements of this Section.

1. Test AND EVALUATION Reports:
2. **[****NFPA 285: Provide documentation from qualified testing agency or fire engineer that the cladding, cladding attachment, insulation, and air barrier system as components of the designed wall assembly have been tested and passed NFPA 285 or approved third-party engineering judgement.]**
3. MANUFACTURER’S INSTRUCTIONS

Provide Manufacturer’s installation instructions for each product specified in this Section.

1. SUSTAINABLE DESIGN SUBMITTALS
2. Submit material health and recycled content of each product specified as required in Quality Assurance Sustainability Standards Certification of this Section.
3. **[LEED: Provide product prerequisite and/or credit summaries for each product specified as applicable including recycled content and Health Product Transparency information.]**
4. SPECIAL PROCEDURE SUBMITTALS

None.

1. QUALIFICATION STATEMENTS

Provide documentation of required Quality Assurance Qualifications for Manufacturers and Installers for all products in wall assembly as required in this Section.

1. WARRANTY DOCUMENTATIOn

Submit sample warranties as required by this Section.

* 1. QUALITY ASSURANCE
1. QUALIFICATIONS
2. MANUFACTURERS

Insulation systems shall be manufactured and marketed by a firm with a minimum of **[20]** years’ experience in the production and sales of insulation materials. Obtain continuous insulation material through one source from a single manufacturer. Manufacturers proposed for use, but not named in these specifications shall submit evidence of ability to meet all requirements specified and include a list of projects of similar design and complexity completed within the past **[five]** years.

1. INSTALLERS

The installation work of this section shall be performed by one entity, an experienced contractor that employs installers and supervisors who are trained and authorized by manufacturer, with a minimum **[two]** years’ record of successful installations on projects of similar scope.

1. CERTIFICATIONS
2. Provide Manufacturer’s written certification that structural system components are compatible.
3. Provide Manufacturer’s written certification that assembly components are compatible with all adjacent materials that come into contact during construction and throughout the life of the building.
4. Provide Manufacturer’s written certification that products are for the intended purpose as described in this Section.
5. SUSTAINABILITY STANDARDS CERTIFICATIONS
6. Minimum recycled content Certified by independent third-party testing.
7. Environmental Product Declaration.
8. **[Cradle to Cradle Material Health Certificate (Mineral Wool Insulation.)]**
9. **[LEED: Provide product prerequisite and/or credit summaries for each product specified as applicable including recycled content and Health Product Transparency information.]**
10. **[UL Certificate Environmental Product Declaration in accordance with ISO 14025.]** [Applies to EcoTouch® Faced and Unfaced Insulation.]
11. **[UL Environment EcoLogo CCD-106.]** [Applies to EcoTouch® Faced and Unfaced Insulation.]
12. **[GREENGUARD Indoor Air Quality Certified® and GREENGUARD Children & School Certified.]** [Applies to EcoTouch® Unfaced Batts and EcoTouch® Faced Batts and Rolls.]
13. **[GREENGUARD Formaldehyde Free.]** [Applies to EcoTouch® Faced and Unfaced Batts and Rolls.]
14. **[Scientific Certification Systems SCS-MC-01025, SCS Certified minimum 65% recycled glass content (with at least 41% post-consumer recycled and the balance of pre-consumer recycled glass content).]** [Applies to EcoTouch® Unfaced Batts and Rolls.]
15. **[Scientific Certification Systems SCS-MC-02676, SCS Certified minimum 58% recycled glass content (with at least 36% post-consumer recycled and the balance of pre-consumer recycled glass content).] [**Applies to EcoTouch® Faced Batts and Rolls.]
16. **USDA Certified Biobased Products: [**Choose one.]
17. **[98%]** [EcoTouch® unfaced]
18. **[57%]** [EcoTouch® Kraft-faced]
19. **[78%]** [EcoTouch® FSK-faced]
20. MOCK-UPS

Construct a wall system sample panel minimum 8 feet long x 8 feet high that includes wood stud framing, sheathing, air and water barrier, mineral wool continuous insulation, insulation fastening methods, through-wall flashing, termination bars, drip edge, sealants, cladding attachment system, **[perimeter fire rated joint],** and cladding. The mock-up shall also include a window, storefront, or door frame, and sill opening transition assembly detailed with lintel, head, and sill flashings, and end dams to demonstrate surface preparation, crack and joint treatment, application of air barriers, and sealing of gaps, terminations, and penetrations of air-barrier assembly.

1. Coordinate construction of mockups to permit inspection by Owner's testing agency of air barrier before external insulation and cladding are installed.
2. Include transitions to roofing membrane, building corner condition, and foundation wall.
3. **[Architect, Engineer, Consultant]** approval of mockup is required. If it is determined that mockup does not comply with requirements, affected details must be reconstructed until mockups are approved.
4. Locate as directed and remove upon review and approval.
5. Approval of mockups does not constitute approval of deviations from the Contract Documents contained in mockups unless **[Architect, Engineer, Consultant]** specifically approves such deviations in writing.
6. **[Indicate portion of wall represented by mockup on Drawings or draw mockup as separate element.]**

[Add note to indicate if ABAA's Quality Assurance Program is required.]

1. **[Subject to compliance with requirements, approved mockups may become part of the completed Work if undisturbed at time of Substantial Completion.]**
2. **[Preconstruction Testing Service: Owner will engage a qualified testing agency to perform preconstruction testing on field mockups.]**
	1. DELIVERY, STORAGE, AND HANDLING
3. Deliver and store products in Manufacturer’s unopened packaging until ready for installation.
4. Store and protect products in accordance with Manufacturer’s instructions. Store in a dry indoor area with adequate ventilation and protect from water, soiling, and direct sunlight.
5. Arrange storage of products to permit access for inspection. Periodically inspect to verify products are undamaged and are maintained in acceptable condition.
6. Remove and replace materials that are damaged.
7. In the event the batt or blanket insulation becomes wet, remove it from the jobsite.
	1. FIELD CONDITIONS
8. AMBIENT CONDITIONS
9. Apply products within the range of ambient and substrate temperatures recommended by manufacturer.
10. Protect substrates from environmental conditions that affect insulation performance
	1. WARRANTY
11. MANUFACTURER WARRANTY
12. Product Warranty

Provide Manufacturer’s standard limited warranty against manufacturing defects.

**PART 2 – PRODUCTS**

* 1. FIBER GLASS BATT INSULATION
1. MANUFACTURERS

BASIS-OF-DESIGN: Owens Corning® ([www.owenscorning.com/insulation/commercial](https://www.owenscorning.com/insulation/commercial)) EcoTouch® Pink® Fiberglas™ Insulation with PureFiber Technology or equal product from one of the following:

1. **[Insert acceptable alternate supplier.]**
2. **[Insert acceptable alternate supplier.]**
3. Substitution Limitations

The “Basis of Design” products listed in this Section are tested and warranted as a system. The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
3. DESCRIPTION

Provide fiber glass batt insulation sized to completely fill the stud cavities.

1. PERFORMANCE/ DESIGN CRITERIA
2. ASTM C665 type **[ I (batt without facing), II Class A (batt with nonreflective facing, flame spread 25 or less), III Class A (batt with reflective facing, flame spread 25 or less)]**
3. **[Noncombustible per ASTM E136.]** [EcoTouch® Unfaced Batt Insulation.]
4. MATERIALS
5. Full width batt for use with wood studs spaced **[16 inches, 24 inches]** on center.
6. Thermal Resistance: Measured in accordance with ASTM C518, R-Value **[13, 15, 19, 21, 30]**.
7. **[Factory-applied facing or Unfaced]:** (If faced, choose from the following options):
8. **[FSK (foil-scrim-kraft, Type III ASTM E84 Class A, Category 1, facer is vapor retarder with 0.02 water vapor Permeance per ASTM E96)].**
9. **[PSK (light-reflective white polypropylene-scrim-kraft, Type II ASTM E84 Class A, Category 1, facer is a vapor retarder with 0.02 water vapor Permeance per ASTM E96)]**

[Do not use unfaced insulation in exposed applications. Kraft and standard foil facings will burn and must not be left exposed. The facing must be installed in substantial contact with the unexposed surface of the ceiling, wall, or floor finish. Protect facing from any open flame or heat source.]

1. Indoor Air Quality: Verified to be formaldehyde free by independent third party such as GreenGuard Environmental Institute, Indoor Air Quality and GreenGuard Gold.
2. Recycled Content: Minimum 50 percent certified by independent third party such as Scientific Certification Systems.
3. Environmental Product Declaration.
4. Declare Label.
5. Sustainable Product Certification: Verified to comply with EcoLogo Certification Criteria Document 016 for Thermal Insulation Materials (CCD-016) for environmentally preferable products.
6. Renewable Materials: Verified to contain renewable ingredients to meet or exceed the biobased content criteria for the USDA Certified Biobased Product Label.
7. ACCESSORIES
8. Tape: polyethylene self-adhering type for Kraft faced insulation and bright aluminum self-adhering type for foil faced insulation.
9. Insulation Fasteners: Impale clip of galvanized steel; type recommended by insulation manufacturer for particular use intended.
10. Mechanical Insulation Fasteners: FM approved, corrosion resistant, size required to suit application.
11. Wire Mesh: Galvanized steel, hexagonal wire mesh.
12. Spindle Fasteners: Corrosion-resistant wire spindles.
	1. MINERAL WOOL BATT INSULATION
13. MANUFACTURERS

BASIS-OF-DESIGN: Owens Corning® ([www.owenscorning.com/insulation/commercial](https://www.owenscorning.com/insulation/commercial)) Thermafiber® UltraBatt™ Mineral Wool Insulation or equal product from one of the following:

1. **[Insert acceptable alternate supplier.]**
2. **[Insert acceptable alternate supplier.]**
3. Substitution Limitations

The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution:

1. Verification that proposed products meet published product performance criteria.
2. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
3. DESCRIPTION

Provide mineral wool batt insulation sized to completely fill the stud cavities.

1. PERFORMANCE/ DESIGN CRITERIA
2. ASTM C665 type **[ I (batt without facing), II Class A (batt with nonreflective facing, flame spread 25 or less), III Class A (batt with reflective facing, flame spread 25 or less)]**
3. MATERIALS
4. Full width batt for use with wood studs spaced **[16 inches, 24 inches]** on center
5. Thermal Resistance: Measured in accordance with ASTM C518, R-Value **[10, 15, 24]**.
6. **[Factory-applied facing or Unfaced]:** (Choose one):
7. **[FSK (foil-scrim-kraft, Type III ASTM E84 Class A, Category 1, facer is vapor retarder with 0.02 water vapor Permeance per ASTM E96)].**
8. **[Unfaced]**
9. Formaldehyde free.
10. Recycled Content: Minimum **[70%, 75%]** percent.
11. NFPA 101: Class A rated interior finish.
12. ASTM C1104: Maximum 1% absorption by volume.

**PART 3 – EXECUTION**

* 1. EXAMINATION
1. Verify that wall, opening framing, bridging and structural bracing, and other framing support members and anchorage have been installed per requirements of the Project.
2. Verify adjacent materials are dry and ready to receive insulation.
3. Verify mechanical and electrical services within walls have been tested and inspected.
4. Do not begin installation until substrates have been properly prepared. If substrate preparation is the responsibility of another installer, notify owner’s agent and **[Architect, Engineer, Consultant]** of unsatisfactory preparation in writing before proceeding. Do not proceed with work until unsatisfactory conditions have been corrected.
5. Installation of products specified in this Section constitutes acceptance of existing conditions and assumption of responsibility for satisfactory performance.
	1. PREPARATION
6. Clean surfaces thoroughly prior to installation.
7. Prepare surfaces using methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	1. INSTALLATION
8. BATT INSULATION
9. Install batt insulation in accordance with manufacturer's recommendations, ASTM C1320, and not before the exterior sheathing has been installed on one side of the stud cavity and sealed to establish complete water resistance.
10. Fit batt insulation tightly into exterior wall wood stud cavity spaces and framing voids to create a continuous insulation layer filling all space in the framing cavity without gaps. Trim to fill spaces and voids neatly. Fluff insulation to full thickness for specified R-value before installation. Do not compress insulation after installation.
11. **[Unfaced, Faced Batt]**: Tightly friction fit full width 16 inches or full width 24 inches batt insulation to fill interior cavity between studs and to completely fill voids inside wood studs.
12. **[Faced Batt]**: Support by friction fit, taping, or adhering facing flanges to face of wood stud. Gypsum board wall finish is applied after facing is secured. No additional support is required.
13. **[Unfaced batt insulation, completely filled cavity depth, both sides of stud cavity closed]**: Friction fit is adequate if insulation completely fills depth of stud cavity and cavity is enclosed on both sides. No additional support is required.
14. **[Unfaced batt insulation, completely filled cavity depth, one side of stud cavity open]**: Friction fit, supplement with straps or wires described below, installed starting at four feet above floor and two feet on center above four feet.
15. **[Supplemental wire or strap supporting devices]**: Multiple types of support devices may be used. Wires shall be inserted through batts extending from stud to stud.
16. **[Wires may be installed continuously through holes in wood stud framing.]**
17. **[Heavy gauge wire may be cut slightly larger than each stud space and wedged into place between studs. When insulation is less than depth of the stud cavity, wires should be positioned to hold batt against the exterior sheathing.]**
18. **[Punched metal straps with pronged tabs shall be attached to the face of the framing and bent 90 degrees pointing into stud cavity and pushed into insulation after installation. The punched prongs shall impale insulation batt to hold it in place.]**

[Choose one]

1. **[Unfaced batt insulation, completely filled cavity depth, one side of stud cavity open]**: Within exterior wall framing, install insulation between pipes, mechanical services, electrical boxes, and backside of exterior sheathing.
2. **[Install factory applied facing with vapor retarder membrane facing building interior. Facing flanges (tabs) may be left unfolded for friction fit installation or may be unfolded and lapped over face of framing members.]**
3. **[Maintain vapor retarder integrity by tightly abutting adjacent insulation. Repair punctures or tears in vapor retarder facing by taping with vapor retarding tape. Follow tape Manufacturer’s application recommendations.]**
	1. REPAIR
4. FILL ERRANT PUNCTURES, PENETRATIONS, AND HOLES
5. **[If vapor barrier facer is damaged leaving penetration into the vapor barrier system, the affected area must be detailed with tape or recommended sealant.]** [Note: Fill of errant punctures, penetrations, and holes may be included in two separate specification sections and therefore the responsibility of two separate trades. Identify the responsible trade according to project specific requirements.]
6. Completely fill the hole with batt insulation to full depth making contact with the back of the sheathing, stud cavity, and fully flush with the outer face of the insulation.
	1. CLEANING
7. Prior to project closeout, remove all related rubbish, excess material, scaffolding, tools, and equipment from the site. Dispose of waste material in a manner approved by applicable jurisdictions.
	1. PROTECTION
8. Protect insulation from damage due to weather and physical abuse until protected by permanent construction.
9. Provide temporary coverings or enclosures where insulation is subject to abuse and cannot be concealed and protected by permanent construction immediately after installation.
10. Touch-up, repair, or replace damaged products before Substantial Completion.

**END OF SECTION 07 21 16**

**SECTION 07 84 00 FIRESTOPPING**

[Include this Part 1- General section for both window/door/opening firestopping and if required for perimeter fire rated joint systems.]

**PART 1 – GENERAL**

* 1. SUMMARY

See Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, Section 01 83 16, **[including mandatory wall system compliance with NFPA 285 (fire spread)].** All proposed product substitutions must comply to be considered.

.

1. SECTION INCLUDES
2. Provide and install wood stud framed exterior wall **[load-bearing, non-load bearing], [fire resistance rated, non-rated]** system, with air and water resistive barrier over the exterior sheathing, with mineral woolcontinuous insulation in the wall cavityand **[faced, unfaced]** **[fiberglass, mineral wool, None]** batt insulation in the stud cavity that effectively controls thermal, air, and water performance and provides continuous insulation and continuity of the building envelope. Provide labor, materials, tools and equipment necessary to complete the Work of this Section including, but not limited to, the following:
	1. Mineral Wool Fire Safing Wall Insulation.
	2. Safing Clips and other accessories to create a continuous perimeter fire containment system as recommended by the Fire Safing Manufacturer.
3. The complete wall system shall include the following:
4. **[Cladding & Cladding Attachment System]** over wood stud framed cavity wall by contractors.
5. Wood framing independently braced cavity to resist vertical and transverse structural loading.
6. Interior gypsum wallboard.
7. **[Faced, Unfaced] [Fiberglass, Mineral Wool]** Insulation batts in the framing cavity
8. Exterior wood sheathing with sealed joints.
9. Continuous air and water resistive barrier system applied to the exterior face of the sheathing wall installed in an airtight and flexible manner, allowing for the relative movement of systems due to thermal and moisture variations and capable of withstanding positive and negative combined wind, stack, and HVAC pressures on the envelope without damage or displacement.
10. Mineral Woolcontinuous insulation preliminarily secured to exterior sheathing with **[screws and air and water sealing washers, impaling pins attached with screws, impaling pins adhesively attached]** and permanently secured with **[cladding attachment system]**.
11. **[Safing to firestop the perimeter of door and window penetrations through wall.]**
12. **[Safing and sealant for sealing gaps between exterior wall and floor edge, perimeter fire containment system.]**
13. All joints, penetrations, and gaps of the air barrier wall system shall be made water and air tight.
14. RELATED SECTIONS

The items listed are not included in this Section, but are specified in the Section listed: [Delete section from the list below that are not required by the project.]

1. **Section 04 42 00 [Project Specific],** Exterior Stone Cladding
2. **Section 05 41 00 [Project Specific],** Structural Metal Stud Framing
3. **Section 05 50 00 [Project Specific],** Metal Fabrication (lintels, shelf angles, and masonry support)
4. **Section 06 11 00 [Project Specific],** Wood Framing
5. **Section 06 16 33 [Project Specific],** Wood Board Sheathing
6. **Section 07 05 43 [Project Specific],** Cladding Support Systems
7. **Section 07 10 00 [Project Specific],** Dampproofing and Waterproofing
8. **Section 07 21 00 [Project Specific],** Thermal Insulation
9. **Section 07 21 13.19 [Project Specific],** Mineral Board Insulation
10. **Section 07 21 16 [Project Specific],** Blanket Insulation
11. **Section 07 27 00 [Project Specific],** Air Barriers
12. **Section 07 42 00 [Project Specific],** Wall Panels
13. **Section 07 44 00 [Project Specific],** Faced Panels
14. **Section 07 46 00 [Project Specific],** Siding
15. **Section 07 50 00 [Project Specific],** Membrane Roofing
16. **Section 07 62 00 [Project Specific],** Sheet Metal Flashing and Trim
17. **Section 07 65 00 [Project Specific],** Flexible Flashings
18. **Section 07 92 00 [Project Specific],** Joint Sealants
19. **Section 09 29 00 [Project Specific],** Gypsum Board
20. **Section xx xx xx [Project Specific],** LEED Requirements

* 1. REFERENCES
1. REFERENCE STANDARDS

Materials shall meet the property requirements of one or more of the following specifications as applicable to the specific product or end use. [Delete references from the list below that are not required by the text of the edited Section.]

1. American Society for Testing of Materials (ASTM)
2. ASTM C272: Standard Test Method for Water Absorption of Core Materials for Structural Sandwich Constructions
3. ASTM C518: Standard Test Method for Steady-State Thermal Transmission Properties by Means of the Heat Flow Meter Apparatus
4. ASTM C553: Standard Specification for Mineral Fiber Blanket Thermal Insulation for Commercial and Industrial Applications
5. ASTM C578: Standard Specification for Rigid Cellular Polystyrene Thermal Insulation
6. ASTM C612: Standard Specification for Mineral Fiber Block and Board Thermal Insulation
7. ASTM C665: Standard Specification for Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction and Manufactured Housing
8. ASTM D1621: Standard Test Method for Compressive Properties of Rigid Cellular Plastics.
9. ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials.
10. ASTM E96: Standard Test Methods for Water Vapor Transmission of Materials
11. ASTM E119: Standard Test Methods for Fire Tests of Building Constructions and Materials
12. ASTM E136: Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750 Degrees C
13. ASTM E331: Standard Test Method for Water Penetration of Exterior Windows, Skylights, Doors and Curtain Walls by Uniform Static Air Pressure Difference
14. ASTM E2307: Standard Test Method for Determining Fire Resistance of Perimeter Fire Barrier Systems Using Intermediate-Scale, Multi-story Test Apparatus
15. ASTM E2393: Standard Practice for On-Site Inspection of Installed Fire Resistive Joint Systems and Perimeter Fire Barriers
16. International Firestop Council
17. National Fire Protection Association (NFPA)
18. NFPA 285: Standard Fire Method for Evaluation of Fire Propagation Characteristics of Exterior Non-Load-Bearing Wall Assemblies Containing Combustible Components
19. NFPA 220: Standard on Types of Building Construction
20. Underwriters Laboratories, Inc. (UL)
21. UL 2079: Tests for Fire Resistance of Building Joint Systems
	1. ADMINISTRATIVE REQUIREMENTS
22. COORDINATION

Coordinate installation of insulation and accessories with sheathing, air barrier membrane, roofing, fenestration, and other moisture protection work.

1. PREINSTALLATION MEETINGS

Convene a meeting of involved sub-contractors a minimum of two weeks prior to commencing Work described in this Section.

1. Attendance is required by representatives of related trades including Owner’s Representative, Contractor, Architect, Installer, Air Barrier Membrane System Manufacturer, Roofing and Foundation Waterproofing Subcontractor, Mechanical Subcontractor, Electrical Subcontractor, and all subcontractors who have materials penetrating the air barrier membrane system or finishes covering the membrane system. Manufacturer’s Representative is available upon request with minimum two-week notice.
2. Contractor shall notify **[Architect, Engineer, Consultant]** at least 14 days prior to time for meeting.
3. Contractor shall record minutes of meeting and distribute to attending parties.
4. The agenda shall include at a minimum:
5. Materials proposed for use.
6. **[Verification of eligibility for any warranty.]**
7. Sequence of construction.
8. Coordination with substrate preparation, condition, and pretreatment.
9. Compatibility of materials.
10. Air barrier requirements and installation.
11. Mechanical and electrical requirements and installation.
12. Minimum curing period.
13. Special details.
14. Mockups.
15. Air leakage and adhesion testing and inspection.
16. Air barrier protection and repair.
17. Work scheduling that covers air barrier coordination with installation of adjacent and covering materials.
18. Review and approval of all glazing applications.
19. Roofing installation.
	1. SUBMITTALS

Provide the following information in accordance with **Section 01 33 00 [Project Specific]** Submittal Procedures.

1. Product Data: Manufacturers’ data on each type of product furnished including:
2. Preparation instructions and recommendations.
3. Technical data and tested physical and performance properties of products.
4. Storage, handling requirements, and recommendations.
5. Shop Drawings (project-specific to air barrier assembly)
6. Show firestopping and sealant layout, profiles, and product components.
7. Include details of interfaces with other materials that form part of air barrier and firestopping.
8. The manufacturer’s engineering judgment drawings must follow requirements set forth by the International Firestop Council.
9. Samples: Submit product samples minimum **[three inch x three inch]** of the following:
10. Mineral wool safing insulation.
11. Any fasteners required to install safing insulation.
12. Certificates:
13. Provide Manufacturer’s written certification that wall assembly components are compatible and provided as a single-source from the manufacturer.
14. Provide Manufacturer’s written certification that wall assembly components are compatible with all adjacent materials that come into contact with the materials during construction and throughout the life of the building.
15. Provide Manufacturer’s written certification that mineral wool safing products are for the intended purpose as described in this Section.
16. Test AND EVALUATION Reports:
17. **[NFPA 285: Provide documentation from qualified testing agency or fire engineer that the cladding, cladding attachment, insulation, and air barrier system as components of the designed wall assembly have been tested and passed NFPA 285 or approved third-party engineering judgement.]**
18. Submit a UL or similar third party tested assembly number, or, if no such information is available, submit a manufacturer’s engineering judgment derived from similar independently tested system designs. The manufacturer’s engineering judgment drawings must follow requirements set forth by the International Firestop Council.
19. Must be submitted to local authorities having jurisdiction for their review and approval prior to installation.
20. MANUFACTURER’S INSTRUCTIONS

Provide Manufacturer’s installation instructions for each product specified in this Section.

1. SUSTAINABLE DESIGN SUBMITTALS

Submit material health and recycled content of each product specified as required in Quality Assurance Sustainability Standards Certification of this Section.

**[LEED: Provide product prerequisite and/or credit summaries for each product specified as applicable including recycled content and Health Product Transparency information.]**

1. SPECIAL PROCEDURE SUBMITTALS

None.

1. QUALIFICATION STATEMENTS

Provide documentation of required Quality Assurance Qualifications for Manufacturers and Installers for all products in tested wall assembly as required in this Section.

1. WARRANTY DOCUMENTATIOn

Submit sample warranties as required by this Section.

* 1. QUALITY ASSURANCE
1. REGULATORY AGENCY SUSTAINABILITY APPROVALS

**[Comply with EPA Preference Program.]**

1. QUALIFICATIONS
2. MANUFACTURERS

Firestopping shall be manufactured and marketed by a firm with a minimum of **[10]** years’ experience in the production and sales of firestopping materials. Obtain firestop material through one source from a single manufacturer. Manufacturers proposed for use, but not named in these specifications shall submit evidence of ability to meet all requirements specified and include a list of projects of similar design and complexity completed within the past **[five]** years.

1. INSTALLERS

The installation work of this section shall be performed by one entity, an experienced contractor that employs installers and supervisors who are trained and authorized by the firestopping manufacturer, with a minimum **[three]** years’ record of successful installations on projects of similar scope. Installer shall designate a single individual as project foreman who shall be on site at all times during installation.

1. CERTIFICATIONS
2. Provide Manufacturer’s written certification that wall assembly components are compatible and provided as a single-source from the manufacturer.
3. Provide Manufacturer’s written certification that wall assembly components are compatible with all adjacent materials that come into contact with the materials during construction and throughout the life of the building.
4. Provide Manufacturer’s written certification that mineral wool safing products are for the intended purpose as described in this Section.
5. Provide certification of Department of Homeland Security SAFETY Act Designation.
6. SUSTAINABILITY STANDARDS CERTIFICATIONS
7. Minimum **[70, 75]** percent recycled content certified by independent third-party testing. [75% required for EPA Preference Program.]
8. Environmental Product Declaration.
9. MOCK-UPS

Construct a wall system sample panel minimum 8 feet long x 8 feet high that includes wood stud framing, sheathing, air and water barrier, mineral wool continuous insulation, insulation fastening methods, through-wall flashing, termination bars, drip edge, sealants, cladding attachment system, **[perimeter fire rated joint],** and cladding. The mock-up shall also include a window, storefront, or door frame, and sill opening transition assembly detailed with lintel, head, and sill flashings, and end dams to demonstrate surface preparation, crack and joint treatment, application of air barriers, and sealing of gaps, terminations, and penetrations of air-barrier assembly.

1. Coordinate construction of mockups to permit inspection by Owner's testing agency of air barrier before external insulation and cladding are installed.
2. Include transitions to roofing membrane, building corner condition, and foundation wall.
3. **[Architect, Engineer, Consultant]** approval of mockup is required. If it is determined that mockup does not comply with requirements, affected details must be reconstructed until mockups are approved.
4. Locate as directed and remove upon review and approval.
5. Approval of mockups does not constitute approval of deviations from the Contract Documents contained in mockups unless **[Architect, Engineer, Consultant]** specifically approves such deviations in writing.
6. **[Indicate portion of wall represented by mockup on Drawings or draw mockup as separate element.]**

[Add note to indicate if ABAA's Quality Assurance Program is required.]

1. **[Subject to compliance with requirements, approved mockups may become part of the completed Work if undisturbed at time of Substantial Completion.]**
2. **[Preconstruction Testing Service: Owner will engage a qualified testing agency to perform preconstruction testing on field mockups.]**
	1. DELIVERY, STORAGE, AND HANDLING
3. Deliver and store products in Manufacturer’s unopened packaging until ready for installation.
4. Store and protect products in accordance with Manufacturer’s instructions. Store in a dry indoor area with adequate ventilation and protect from water, soiling, and direct sunlight.
5. Arrange storage of products to permit access for inspection. Periodically inspect to verify products are undamaged and are maintained in acceptable condition.
6. Remove and replace materials that are damaged.
	1. FIELD CONDITIONS
7. AMBIENT CONDITIONS
8. Apply products within the range of ambient and substrate temperatures recommended by manufacturer.
9. Protect substrates from environmental conditions that affect insulation performance
	1. WARRANTY
10. MANUFACTURER WARRANTY
11. Product Warranty

Provide Manufacturer’s standard limited warranty against manufacturing defects.

**PART 2 – Products**

[Use from Section 07 84 13 or Section 07 84 53.]

**PART 3 – Execution**

[Use from Section 07 84 13 or Section 07 84 53.]

**END OF SECTION 07 84 00**

**SECTION 07 84 13 PENETRATION FIRESTOPPING**

[Include this section for window/door/opening firestopping if required.]

**PART 1 – GENERAL**

[Use the General Section from Section 07 84 00.]

**PART 2 – PRODUCTS**

* 1. SAFING INSULATION
1. MANUFACTURERS

BASIS-OF-DESIGN: Owens Corning® ([www.owenscorning.com/insulation/commercial](https://www.owenscorning.com/insulation/commercial)) Thermafiber® Safing Insulation or equal product from one of the following:

1. **[Insert acceptable alternate supplier.]**
2. **[Insert acceptable alternate supplier.]**
3. Substitution Limitations

The “Basis of Design” products listed in this Section are tested and warranted as a system.  The Contractor shall provide the products of the named manufacturers without substitution, unless a written request for an “or equal complete system substitution” has been approved in writing by the **[Architect, Engineer, Consultant]**. Substitution requests must be accompanied by the following to be considered for substitution.

1. Verification that proposed products meet published product performance criteria.
2. Verification from the proposed manufacturers of independent third-party listings or engineering judgements that the proposed system substitution meets the **[NFPA 285 (fire propagation)]**, the **[ASTM E119 (fire resistance)]** requirements.
3. Verification from proposed manufacturers that the proposed substitution is tested with the other assembly components to meet Division 01, EXTERIOR ENCLOSURE PERFORMANCE REQUIREMENTS, **Section 01 83 16 [Project Specific].**
4. DESCRIPTION

Provide safing insulation for gaps around the perimeter of openings, penetrations, and the perimeter edge of floor assemblies and non-fire-resistance rated exterior curtain walls as shown in NFPA 285 detail drawings. Each insulation board must be labeled with manufacturer's name, product brand name, ASTM material specification reference, and identification of the third-party inspection agency used for building code qualification.

1. PERFORMANCE/ DESIGN CRITERIA
2. Provide mineral wool safing in compliance with ASTM C612, Type IA, IB and II.
3. Designated Type SAF in UL Fire Resistance Directory.
4. Surface-Burning Characteristics: Tested in accordance with ASTM E84
5. **[Unfaced: Maximum flame spread 0 and smoke-developed of 0]**
6. **[Foil Faced: Maximum flame spread 25 and smoke-developed of 0]**
7. MATERIALS
8. R-Value: 4.3 per inch
9. Facing: [**Unfaced, Foil Faced]**
10. Density: [**4.0 pcf (actual), 6.0 pcf (actual)]** [Minimum thickness and density as noted in tested and listed design.]
11. Fiber Type: Standard fiber; minimum 70% **[75% pre-consumer recycled content; complies with EPA Preference Program]**.
12. Post-Consumer Recycled Content: 0%.
13. Department of Homeland Security SAFETY Act Designation: Qualifies.

**PART 3 – EXECUTION**

* 1. EXAMINATION
1. Verify that wall, opening framing, bridging and structural bracing, and other framing support members and anchorage have been installed per requirements of the Project.
2. Verify adjacent materials are dry and ready to receive insulation.
3. Verify that substrates are sound and free of oil, grease, dirt, excess mortar, or other contaminants.
4. Do not begin installation until substrates have been properly prepared. If substrate preparation is the responsibility of another installer, notify owner’s agent and **[Architect, Engineer, Consultant]** of unsatisfactory preparation in writing before proceeding. Do not proceed with work until unsatisfactory conditions have been corrected.
5. Installation of products specified in this Section constitutes acceptance of existing conditions and assumption of responsibility for satisfactory performance.
	1. PREPARATION
6. Prepare surfaces using methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	1. INSTALLATION
7. SAFING INSULATION
8. For fluid-applied air & water resistive barrier system, verify manufacturer recommended cure time before installing fire safing insulation**.**
9. Install safing batt in sections a minimum four inch wide, stacked to a thickness that is a minimum of 25 percent greater than the width of the gap between the back of the masonry veneer and the face of the wood stud framed wall to achieve a minimum 25 percent compression and tight friction fit after installation.
10. Install Safing insulation compressed in the thickness direction and flush with the edge of the opening.
11. Install Safing insulation in maximum sizes to minimize joints.
12. Safing insulation edges shall be butted together tightly and fit around openings and penetrations. Install square edges to fit square and tight.
13. Extend insulation in thickness indicated to envelop entire area to be insulated. Cut and fit tightly around obstructions and fill voids with insulation. Remove projections that interfere with placement.
14. Safing shall be tightly butted at ends of adjacent pieces to completely close the air space behind the cladding.
15. Install exterior cladding as soon as possible, best within 60 days.
	1. REPAIR
16. FILL ERRANT PUNCTURES, PENETRATIONS, AND HOLES
17. If fasteners are removed or where holes are drilled into mineral wool insulation, the affected area must be detailed with air barrier sealant see **[Section 07 27 00 Air Barriers- Project Specific]**
18. Completely fill the hole with Safing. Fill the hole in the insulation to full depth making contact with the air and water barrier membrane below the insulation and fully flush with the outer face of the insulation.
	1. FIELD INSPECTION

Follow criteria outlined in ASTM E2393 Standard Practice for On-Site Inspection of Installed Fire Resistive Joint Systems and Perimeter Fire Barriers.

* 1. CLEANING
1. Prior to project closeout, remove all related rubbish, excess material, scaffolding, tools, and equipment from the site. Dispose of waste material in a manner approved by applicable jurisdictions.
	1. PROTECTION
2. Protect installed products until completion and project closeout.
3. Touch-up, repair, or replace damaged products before Substantial Completion.

**END OF SECTION 07 84 13**

Pub No 10023858-A. The color PINK is a registered trademark of Owens Corning. © 2019 Owens Corning. All Rights Reserved. ® 2019 Thermafiber, Inc. All Rights Reserved. Trademarks are the properties of their respective owners.